# RIM2D model definition — v1
# Grid: 2418 x 2219
# Written by hazard-model-api/prepare_rim2d_case.py

###### INPUT RASTERS ######
**DEM**
input/dem.nc
**buildings**
input/buildings.nc
**IWD**
file
input/iwd.nc
**roughness**
file
input/roughness.nc
**pervious_surface**
input/pervious_surface.nc
**sealed_surface**
input/sealed_surface.nc
**sewershed**
input/sewershed.nc

###### RAINFALL ######
**pluvial_raster_nr**
240
**pluvial_dt**
1800
**pluvial_start**
0
**pluvial_base_fn**
../input/rain/imerg_t

###### OUTPUT ######
**output_base_fn**
output/case_v1_
**out_cells**
input/outflowlocs.txt
**out_timing_nr**
240
**out_timing**
1800 3600 5400 7200 9000 10800 12600 14400 16200 18000 19800 21600 23400 25200 27000 28800 30600 32400 34200 36000 37800 39600 41400 43200 45000 46800 48600 50400 52200 54000 55800 57600 59400 61200 63000 64800 66600 68400 70200 72000 73800 75600 77400 79200 81000 82800 84600 86400 88200 90000 91800 93600 95400 97200 99000 100800 102600 104400 106200 108000 109800 111600 113400 115200 117000 118800 120600 122400 124200 126000 127800 129600 131400 133200 135000 136800 138600 140400 142200 144000 145800 147600 149400 151200 153000 154800 156600 158400 160200 162000 163800 165600 167400 169200 171000 172800 174600 176400 178200 180000 181800 183600 185400 187200 189000 190800 192600 194400 196200 198000 199800 201600 203400 205200 207000 208800 210600 212400 214200 216000 217800 219600 221400 223200 225000 226800 228600 230400 232200 234000 235800 237600 239400 241200 243000 244800 246600 248400 250200 252000 253800 255600 257400 259200 261000 262800 264600 266400 268200 270000 271800 273600 275400 277200 279000 280800 282600 284400 286200 288000 289800 291600 293400 295200 297000 298800 300600 302400 304200 306000 307800 309600 311400 313200 315000 316800 318600 320400 322200 324000 325800 327600 329400 331200 333000 334800 336600 338400 340200 342000 343800 345600 347400 349200 351000 352800 354600 356400 358200 360000 361800 363600 365400 367200 369000 370800 372600 374400 376200 378000 379800 381600 383400 385200 387000 388800 390600 392400 394200 396000 397800 399600 401400 403200 405000 406800 408600 410400 412200 414000 415800 417600 419400 421200 423000 424800 426600 428400 430200 432000

###### MODEL PARAMETERS ######
**dt**
1
**sim_dur**
432000
**inf_rate**
0
**sewer_cap**
0
**sewer_threshold**
0.002
**alpha**
0.4
**theta**
0.8

###### FLAGS ######
**verbose**
.TRUE.
**routing**
.TRUE.
**superverbose**
.FALSE.
**neg_wd_corr**
.TRUE.
**sew_sub**
.FALSE.
none
**fluv_bound**
.FALSE.
**full_out**
.FALSE.
**closed_boundaries**
.FALSE.
**sheetflow_roughness**
.TRUE.

**fluvial_boundary**
input/fluvial_boundary_none.txt

# end
